Reception window

Data packet

Acknowledgement packet

Send data packets until ACK received

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  | D | D | D | | D | A |  |  | |  | | D | |
| Sender |  |  |  |  |  | |  |  |  |  | |  | | A | |
|  |  |  |  |  | |  | D | A |  | |  | |  | |  |

Receiver

Transmission detected